	Category C1/D1 Safety Questions 

	 Question
	             Topic
	Show
/ Tell
	                                                            Question
	
	                                                                  Answer

	C1
	Doors
	Show
	Show me how you check that all doors including cargo doors are secure.
	
	All doors must be closed and locking levers for cargo doors are set in the recommended secured position.

	C2
	Air 
	Show
	Show me how you would check for air leaks on this vehicle.
	
	Charge the air tanks; consult gauges for drops in air pressure. Walk round the vehicle listening for any obvious leaks.

	C3

	Loading
	Tell
	Tell the main safety factors involved in loading this vehicle.
	
	The load should be evenly distributed throughout the length of the vehicle so as not to affect control while the vehicle is being driven. Any load must be carried so that it does not endanger other road users. It must securely stowed within the size and weight limits for the vehicle. The load needs to be secure so that it cannot move or fall from the vehicle when cornering or braking.

	C4
	Body
	Tell
	Tell me how you would check the condition of the reflectors on this vehicle.
	
	Ensure that all reflectors are fitted, clean, and functional (not cracked or broken).

	C5


	Windscreen
	Tell
	Tell me how you would check the condition of the windscreen and windows on this vehicle.
	
	The windscreen and windows must be clean, clear and free from defects. No mascots or stickers that restrict view.

	C6


	Mudguards
	Show
	Show me how you would check the condition of the mudguards on this vehicle.
	
	As part of the daily walk-round check ensure mudguards and spray suppression equipment are secure.
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	C7
	Tyres
	Tell 
	Tell me how you would check your tyres to ensure that they are correctly inflated, have sufficient tread depth and that their general condition is safe to use on the road.
	
	Follow the manufacturer’s guide, using appropriate equipment, check and adjust pressures when tyres are cold. Must have a tread depth of at least 1mm across ¾ of the breadth of the tread and in a continuous band around the entire circumference. There should be no cuts, damage or signs of cord visible at the sidewalls.

	C8


	Windscreen
Wipers
	Tell
	Tell me how you would check the condition of the windscreen wipers on this vehicle.
	
	The windscreen wipers must operate. Blades should be in good condition.

	C9





	Body
	Tell
	Tell me how you would check the condition of the body is safe on this vehicle.
	
	As part of a daily walk-round check, ensure the
body is fully roadworthy and there are no significant defects. No loose panels or items, which could endanger other road users. All inspection panels must be secure.

	C10



	Air
	show
	Show me how you would check for the correct air pressure on this vehicle.
	
	Ensure gauges are reading the correct pressures for the vehicle and that all warning lights are extinguished and audible warning devices are not sounding.

	C11
	Oil
	Show
	Identify where you would check the engine oil level and tell me how you would check that the engine has sufficient oil.
	
	Identify dipstick / oil level indicator. Describe check of oil against the minimum/maximum markers.


	C12
	Wheel Nuts
	Show
	Show me how you would check that the wheel
nuts are secure on this vehicle.
	
	A visual check to identify any nuts that are
obviously loose, and check that the wheel nut
indicators (if fitted) are in alignment.
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	C13
	Horn
	Show
	Show me how you would check the operation (specify horn, warning device for reversing) of audible warning devices on this vehicle.
	
	Demonstrate use of control.

	C14
	Suspension
	Tell
	Tell me how you would check the condition of the suspension on this vehicle.
	
	As part of a daily walk-round check, suspension should be checked for any obvious signs of deterioration or damage.

	C15
	Brake lights
	Show
	Show me how you would check the brake lights are working on this vehicle. (I can assist you, if you need to put the ignition on, please don’t start the engine).
	
	Operate the brake pedal, make use of reflections in windows, garage doors, etc, or ask someone to help.

	C16
	Coolant
	Show
	Identify where you would check the engine coolant level and tell me how you would check that the engine has the correct level.
	
	Identify high/low level markings on the header tank where fitted or radiator filler cap, and describe how to top up level.


	C17
	Lights
	Tell
	Tell me how you would check that the Headlamp. Sidelights and tail lights are working.
	
	Explain: Operate switch (turn on ignition if necessary), walk round vehicle

	C18
	Tacho
	Show
	Show me how you replace the tachograph disc on this vehicle
	
	Candidate to demonstrate how to insert tachograph disc. Digital tachographs may require an explanation if candidate does not have a digital card.
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	C19


	Loading
	Tell
	Tell me how you would operate the loading
Mechanism on this vehicle (Vehicle specific. e.g. Tail Lift).
	
	Candidates should be able to explain briefly the
correct operation and safe working practice of
specific machinery fitted to the vehicle, e.g. tail
lift, kneeling bus.

	C20
	Steering
	Show
	Show me / Explain how you check that the power assisted steering is working.
	
	If the steering becomes heavy the system may not be working properly. Before starting a journey two simple checks can be made. Gentle pressure on the steering wheel, maintained while the engine is started, should result in a slight noticeable movement as the system begins to operate. Alternatively turning the steering wheel just after moving off will give an immediate indication that the power assistance is functioning.

	C21
	Indicators
	Show
	Show me how you would check the Directional indicators are working.
	
	Apply the indicators or hazard warning switch and check function of all indicators.

	C22
	Windscreen Washer
	Show
	Identify where the windscreen washer reservoir is and tell me how you would check the windscreen washer level.
	
	Identify reservoir and explain how to check level.


	C23
	Instruments
	Show
	Show me what instrument checks you would make before and after starting the engine on this vehicle.
	
	Check to make sure all gauges and warning systems are working. Ensure that all gauges are reading correctly and that warning lights / audible warning devices are extinguished before moving away.

	C24
	First Aid
	Show
	Show me where the first aid equipment is kept on this vehicle.
	
	Candidate to indicate equipment if carried. Where equipment is not carried, candidates should be able to explain under what circumstances (i.e. vehicle types, loads carried) it must be provided 
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	C25
	Windscreen
Washers
	Show
	Show me how you would clean the windscreen using the windscreen washers and wipers.
	
	Operate control to wash and wipe windscreen (turn ignition on if necessary)

	C26
	Windscreen
Demister
	Show
	Show me how you would set the windscreen demister to clear the windows effectively.

	
	Set all relevant controls including: fan, temperature, air direction/ source and heated screen to clear windscreen and windows. Engine does not have to be started for this.

	C27

	Rear Fog Light
	Show
	Show me how you switch on the rear fog light(s) and explain when you would use them. (No need to exit the vehicle)
	
	Operate switch (turn on ignition and dipped headlights if necessary). Check warning light is on. Explain use i.e. when visibility is reduced to less than 100 metres.

	E16

	Headlights
	Show
	Show me hoe you switch your headlights from dipped to main beam.
	
	Operate switch (with ignition or engine on if necessary). Check with main beam warning light is on. 

	E17

	Brake lights
	show
	Show me how you would check the brake lights are working on this vehicle. (I can assist you, if you need to put the ignition on, please don’t start the engine).
	
	Operate the brake pedal, make use of reflections in windows, garage doors, etc, or ask someone to help.

	
	
	
	
	
	

	
	
	
	
	
	

	Question covered by procedures already in place will continue to be asked as at present.  These will be in addition to the combination used on test.

	Are you satisfied that your cab locking mechanism is secure?

	Show me where the emergency exits are and how you would check that they are operating correctly. 










































