	 Category B + E Safety Questions 

	 Question
	             Topic
	Show
/ Tell
	                                                            Question
	
	                                                                  Answer

	BE1
	Brake Fluid
	Show 
	Open the bonnet, identify where the brake fluid reservoir is and tell me how you would check that you have a safe level of hydraulic brake fluid.	
	
	Identify reservoir, check level against high/low markings

	BE2
	Indicators
	Show
	Show me how you would check the Directional indicators are working.
	
	Apply the indicators or hazard warning switch and check function of all indicators.

	BE3
	Loading
	Tell
	[bookmark: _GoBack]Tell the main safety factors involved in loading this vehicle.1
	
	The load should be evenly distributed throughout the trailer. Heavy items should be loaded as low as possible so that they are mainly over the axle(s). Bulkier, lighter items should be distributed to give a suitable ‘nose weight’ at the towing coupling. The nose weight should never exceed the vehicle manufacturer’s specifications.

	BE4
	Loading
	Tell
	Tell the main safety factors involved in securing a load on this vehicle.
	
	 Any load must be carried so that it does not endanger other road users. It must securely stowed within the size and weight limits for the vehicle. The load needs to be secure so that it cannot move or fall from the vehicle when cornering or braking.

	BE5
	Doors
	Show
	Show me how you check that your vehicle & trailer doors are secure.
	
	Physical checks should be made to ensure that windows, roof light and all doors, including cargo doors are properly closed.

	BE6
	Tyres
	Tell 
	Tell me how you would check your tyres to ensure that they have sufficient tread depth and that their general condition is safe to use on the road.
	
	No cuts or bulges, 1.6mm of tread depth across ¾ of the breath of the tyre and around the entire circumference. Check tyre pressures

	BE7
	Horn
	Show
	Show me how you would check that the horn is working (off road only).
	
	Check is carried out by using control (turn on ignition if necessary).
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	BE8
	Engine coolant
	Show 
	Open the bonnet, identify where you would check the engine coolant level and tell me how you would check that the engine has the correct level.	
	
	Identify high/low level markings on the header tank where fitted or radiator filler cap, and describe how to top up level.


	BE9


	Handbrake
	Show
	Show me how you check the parking brake for excessive wear.
	
	Demonstrate by applying parking brake that when it is fully applied it secures itself, and is not at the end of the working travel.

	BE10

	Windscreen
Washers
	Show
	Show me how you would clean the windscreen using the windscreen washers and wipers.
	
	Operate control to wash and wipe windscreen (turn ignition on if necessary).

	BE11



	Windscreen
Demister
	Show
	Show me how you would set the windscreen demister to clear all the windows effectively, this should include both front and rear screens. 
	
	Set all relevant controls including: fan, temperature, air direction/ source and heated screen to clear windscreen and windows. Engine does not have to be started for this.

	BE12
	Rear Fog Light
	Show
	Show me how you switch on the rear fog light(s) and explain when you would use them. (No need to exit the vehicle)
	
	Operate switch (turn on ignition and dipped headlights if necessary). Check warning light is on. Explain use i.e. when visibility is reduced to less than 100 metres.

	BE13
	Headlights
	Show
	Show me how you switch your headlights from dipped to main beam and explain how you would know main beam is on whilst inside the car.
	
	Operate switch (with ignition or engine on if necessary). Check with main beam warning light is on. 

	 BE14
	Brake lights
	Show
	Show me how you would check the brake lights are working on this vehicle. (I can assist you, if you need to put the ignition on, please don’t start the engine).
	
	Operate the brake pedal, make use of reflections in windows, garage doors, etc, or ask someone to help.

	BE15
	Head Restraints
	Tell
	Tell me how you make sure your head restraint is correctly adjusted so it provides the best protection in the event of a crash.
	
	The head restraint should be adjusted so the rigid part of the head restraint is at least as high as the eye or top of the ears, and as close to the back of the head as is comfortable.  Some restraints might not be adjustable.



