[bookmark: _GoBack]CUNCOUPLE THE TRAILER

1. Apply Parking Brake
2. Remove Electrics (stow away)
3. Wind down Jockey a few turns first then release and drop to the floor then retighten
4. Open Hitch coupling and at the same wind up Jockey wheel to raise Hitch from the Tow Ball
5. Check Brake operation by giving a quick shove
6. Remove Trailer breakaway Cable
7. Remove Number plate (If Required) 

TO COUPLE UP THE TRAILER

Carry out check of trailer to ensure its fit to go on the road
Start at the front and check the following:
Parking brake works (Give Trailer a push)                  Tow hitch		Gaitor (no splits in it)
Trailer Breakaway cable		Jockey Wheel (wind up/down)		Electrics (no baring wires)     Lights (secure/clean)	              Body secure                                                   Reflectors	
Tyres (min 1.6mm Tread)	wheel arches		                              wheel nuts
Doors secure      Fit matching Number Plate

POSITION VEHICLE INFRONT OF TRAILER (stop about 1 ½  meter away)  Check height of hitch, back into position
COUPLING UP THE TRAILER.
1. Fit Trailer Breakaway Cable
2. Using Jockey wheel lower Hitch onto ball until secure ( CONFIRM BY WINDING BACK UP)
3. Secure jockey wheel away
4. Fit Electrics
5. Release Parking Brake
6. Check Electrics work

